/timing/S00_Entry/MMU_REGSLICE/value=1;range=0,1;strength=0
/functional/S00_Entry/SUPPORTS_DECERR/value=1;range=0,1;strength=0
/functional/S00_Entry/SUPPORTS_WRAP/value=1;range=0,1;strength=0
/timing/S00_Entry/TR_REGSLICE/value=1;range=0,1;strength=0
/timing/S00_Buffer/AR_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/AR_M_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/AR_M_SEND_PIPE/value=1;range=0,1;strength=0
/timing/S00_Buffer/AR_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/timing/S00_Buffer/AW_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/AW_M_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/AW_M_SEND_PIPE/value=1;range=0,1;strength=0
/timing/S00_Buffer/AW_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/timing/S00_Buffer/B_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/B_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/timing/S00_Buffer/R_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/R_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/timing/S00_Buffer/W_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/W_M_PIPE/value=0;range=0..8;strength=0
/timing/S00_Buffer/W_M_SEND_PIPE/value=1;range=0,1;strength=0
/timing/S00_Buffer/W_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/config/S00_Entry/DATA_WIDTH/value=32;annotatable=1
/config/S00_Entry/ID_WIDTH/value=0;annotatable=1
/config/S00_Entry/PROTOCOL/value=AXI4;annotatable=1
/config/S00_Entry/ADDR_WIDTH/value=36;annotatable=1
/timing/S01_Entry/MMU_REGSLICE/value=1;range=0,1;strength=0
/functional/S01_Entry/SUPPORTS_DECERR/value=1;range=0,1;strength=0
/functional/S01_Entry/SUPPORTS_WRAP/value=1;range=0,1;strength=0
/timing/S01_Entry/TR_REGSLICE/value=1;range=0,1;strength=0
/timing/S01_Buffer/AR_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S01_Buffer/AR_M_PIPE/value=0;range=0..8;strength=0
/timing/S01_Buffer/AR_M_SEND_PIPE/value=1;range=0,1;strength=0
/timing/S01_Buffer/AR_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/timing/S01_Buffer/R_SLR_PIPE/value=0;range=0..8;strength=0
/timing/S01_Buffer/R_SYNC_STAGES/value=3;range=2,3,4,5,6,7,8;strength=0
/config/S01_Entry/DATA_WIDTH/value=32;annotatable=1
/config/S01_Entry/ID_WIDTH/value=0;annotatable=1
/config/S01_Entry/PROTOCOL/value=AXI4;annotatable=1
/config/S01_Entry/ADDR_WIDTH/value=36;annotatable=1
/timing/M00_Buffer/AR_SLR_PIPE/value=0;range=0..8;strength=0
/timing/M00_Buffer/AW_SLR_PIPE/value=0;range=0..8;strength=0
/timing/M00_Buffer/B_SLR_PIPE/value=0;range=0..8;strength=0
/timing/M00_Buffer/B_M_PIPE/value=0;range=0..8;strength=0
/timing/M00_Buffer/B_M_SEND_PIPE/value=1;range=0,1;strength=0
/timing/M00_Buffer/R_SLR_PIPE/value=0;range=0..8;strength=0
/timing/M00_Buffer/R_M_PIPE/value=0;range=0..8;strength=0
/timing/M00_Buffer/R_M_SEND_PIPE/value=1;range=0,1;strength=0
/timing/M00_Buffer/W_SLR_PIPE/value=0;range=0..8;strength=0
/timing/M00_Exit/REGSLICE/value=1;range=0,1;strength=0
/config/M00_Exit/DATA_WIDTH/value=64
/config/M00_Exit/ID_WIDTH/value=4
/config/M00_Exit/PROTOCOL/value=AXI4
/config/M00_Exit/ADDR_WIDTH/value=32
/timing/SW0/AR_M_PIPE/value=1;range=0..8;strength=0
/timing/SW0/AR_S_PIPE/value=0;range=0..8;strength=0
/timing/SW0/AW_M_PIPE/value=1;range=0..8;strength=0
/timing/SW0/AW_S_PIPE/value=0;range=0..8;strength=0
/timing/SW0/B_M_PIPE/value=1;range=0..8;strength=0
/timing/SW0/B_S_PIPE/value=0;range=0..8;strength=0
/timing/SW0/R_M_PIPE/value=1;range=0..8;strength=0
/timing/SW0/R_S_PIPE/value=0;range=0..8;strength=0
/timing/SW0/W_M_PIPE/value=1;range=0..8;strength=0
/timing/SW0/W_S_PIPE/value=0;range=0..8;strength=0
/config/ip/num_si/value=2
/config/ip/num_mi/value=1
/config/ip/num_clks/value=2
/config/aclk/csk/value=design_1_mig_7series_0_0_ui_clk:200:0
/clocking/M00_Exit/ASSOCIATED_CLK/value=aclk;range=aclk;editable=0
/config/aclk1/csk/value=_clk_wiz_0_clk_out1:100:0.0
/clocking/S00_Entry/ASSOCIATED_CLK/value=aclk1;range=aclk1;editable=0
/clocking/S01_Entry/ASSOCIATED_CLK/value=aclk1;range=aclk1;editable=0
/clocking/SW0/ASSOCIATED_CLK/value=aclk;range=aclk,aclk1;strength=0
/functional/S00_Entry/LIM_R_LEN/value=0;range=0,1,2,4;strength=0
/functional/S00_Entry/LIM_W_LEN/value=0;range=0,1,2,4;strength=0
/functional/S00_Entry/PKT_R_THR/value=0;range=0,1,2,4,8,16,32;strength=0
/functional/S00_Entry/PKT_W_THR/value=0;range=0,1,2,4,8,16,32;strength=0
/functional/S01_Entry/LIM_R_LEN/value=0;range=0,1,2,4,8;strength=0
/functional/S01_Entry/PKT_R_THR/value=0;range=0,1,2,4,8,16,32;strength=0
/functional/SW0/DATA_WIDTH/value=64;range=32,64,128,256,512,1024;strength=0
/functional/M00_Buffer/AR_SIZE/value=32;range=0,1,2,4,8,16,32;strength=0
/functional/M00_Buffer/AW_SIZE/value=32;range=0,1,2,4,8,16,32;strength=0
/functional/M00_Buffer/B_SIZE/value=32;range=0,1,2,4,8,16,32;strength=0
/functional/M00_Buffer/R_SIZE/value=32;range=0,1,2,4,8,16,32,64,128,256,512,1024,2048,4096;strength=0
/functional/M00_Buffer/W_SIZE/value=32;range=0,1,2,4,8,16,32,64,128,256,512,1024,2048,4096;strength=0
/functional/S00_Buffer/AR_SIZE/value=32;range=16,32;strength=0
/functional/S00_Buffer/AW_SIZE/value=32;range=16,32;strength=0
/functional/S00_Buffer/B_SIZE/value=32;range=16,32;strength=0
/functional/S00_Buffer/R_SIZE/value=32;range=16,32,64,128,256,512,1024,2048,4096;strength=0
/functional/S00_Buffer/W_SIZE/value=32;range=16,32,64,128,256,512,1024,2048,4096;strength=0
/functional/S01_Buffer/AR_SIZE/value=32;range=16,32;strength=0
/functional/S01_Buffer/R_SIZE/value=32;range=16,32,64,128,256,512,1024,2048,4096;strength=0
